**Product: JBL Synthesis SCL-6**

**Description Title:** SCL-6

**Descriptor:** 2.5-Way Quadruple 5.25-inch (130mm) In-Wall Loudspeaker

**Short Descriptor:** 2.5-Way Quadruple 5.25-inch (130mm) In-Wall Loudspeaker

**Short Description:** The SCL-6 is the largest in-wall model in the expanded JBL Synthesis Custom Loudspeaker (SCL) series. It is designed for deployment in high-performance immersive audio systems in medium to large size rooms. The SCL-6 features JBL’s patented 2410H-2 1-inch (25mm) compression driver mated to a High Definition Imaging (HDI™) horn. This patented horn design is integrated with four 5.25-inch (130 mm) Advanced Aluminum Matrix cone cast-frame woofers into a precision molded baffle assembly. The configuration yields incredibly smooth and consistent performance for in-wall LCR or surround applications. The SCL-6 is acoustically designed to match any of the JBL Synthesis Custom Loudspeakers (SCL series) as part of a complete JBL Synthesis immersive audio solution.

**Long Description:** The SCL-6 is the largest in-wall model in the expanded in the JBL Synthesis Custom Loudspeaker (SCL) series. It is designed for deployment in high-performance immersive audio systems in medium to large size rooms. The SCL-6 features JBL’s patented 2410H-2 1-inch (25mm) compression driver mated to a High Definition Imaging (HDI™) horn. This patented horn design is integrated with four 5.25-inch (130mm) Advanced Aluminum Matrix cone cast-frame woofers into a precision molded baffle assembly. The configuration yields incredibly smooth and consistent performance for in-wall LCR or surround applications. Premium components are used throughout the crossover network including a boundary gain adjustment switch while high-quality gold-plated push type speaker terminals ensure a secure connection. Installation is simple and quick with the new Cat Claw mounting mechanism that allows the speaker to be securely clicked into place freeing up two hands for tightening it down flush and level to the wall. A zero bezel magnetically attached grille is included and can be painted to match any décor. The SCL-6 is acoustically designed to match any of the JBL Synthesis Custom Loudspeakers (SCL series) as part of a complete JBL Synthesis immersive audio solution.

**Highlights:**

* 2.5-way in-wall loudspeaker system designed for on-axis listening as LCR and surround channels
* 1-inch 2410H-2 compression driver tweeter mated to a JBL patented High-Definition Imaging (HDI™) horn precision molded baffle assembly
* Four 5.25-inch (130mm) Advanced Aluminum Matrix cone cast frame woofers
* Can be mounted vertically or horizontally
* Patented Cat Claw installation mechanism
* Gold plated, spring-loaded binding posts
* Includes paintable zero-bezel, magnetically attached grilles
* Compatible with WB54 pre-construction bracket

**General Specifications:**

|  |  |
| --- | --- |
| Type: | 2.5-Way In-wall loudspeaker |
| Low Frequency Driver: | Four 5.25” (130 mm) advanced Aluminum Matrix cone cast-frame woofers (JW13Al-4) |
| High Frequency Driver: | 1" (25 mm) 2410H-2 Teonex® annular ring-diaphragm compression driver |
| Recommended Amplifier Power: | 25 – 200W RMS |
| Impedance: | 4 Ohm |
| Loudspeaker Sensitivity: | 91 dB/2.83V/1m |
| Frequency Response: | 50Hz - 30kHz (-6 dB on-axis), 2pi anechoic |
| Crossover Frequency: | 1.8 kHz |
| High Frequency Coverage Angle (-6 dB): | 80° Vertical / 80° Horizontal, from 2 kHz to 17 kHz. |
| Enclosure Type: | Open back |
| Controls: | Boundary Proximity Control |
| Grille Dimensions: | 7.29” (185 mm) x 31.32” (796 mm) |
| Product Dimensions (with grille): | 7.29” (185 mm) x 31.32” (796 mm) x 3.82” (97.1 mm) |
| Cut-out Dimensions: | 5.95” (151 mm) x 29.98” (761 mm) |
| Rough-in Bracket: | WB54 |
| Mounting Depth: | 3.63” (92 mm) |
| Input Type | Gold-plated spring-loaded binding posts |
| Product Weight: | 22.2 lbs (10.07 kg) |
| Shipping Weight: | 25.6 lbs (11.61 kg) |
| Shipping Units of Measure: | Each |
| Warranty: | 5 Years |

**Web Product Page Attachments:**

* Owner’s Manual
* Spec Sheet
* Quick Specs
* WB54 Quick Specs